Cambridge Bus Compressor v1.0.0
================================

Classic Bus Glue.

Initial release highlights
- Calibrated bus-compressor model with 20 factory presets.
- Stereo Linked, independent L/R, and M/S routing.
- Stereo Linked uses lane A as the single runtime authority for compressor
  controls and crossover on both channels; stored lane B settings resume when
  routing is unlinked.
- Independent lane/band control with asymmetric multiband layouts.
- Processor-owned Auto GR with editor-open/headless equivalence.
- Auto GR disengage commits both effective Threshold and level-restoring Gain,
  preserving the manual handoff without a level jump.
- While Auto GR is active, the GAIN control follows the effective live makeup
  offset without writing host automation or changing the stored manual value.
- Manual GAIN drag, typed-value, and default gestures during Auto GR target
  the displayed effective Gain without double-counting the live makeup offset.
- Visible Mode, Detector Mode, external sidechain, sidechain-listen, and
  routing-aware Listen controls, synchronized with host automation and state.
- Per-channel metering, bypass/state synchronization, and deterministic recall.
- Fixed native-rate 1x processing with zero oversampling latency.
- VST3 and CLAP formats.
- Free product: no licence, activation, trial, demo interruption, or network use.

Documentation status
The approved Cambridge Bus Compressor User Manual and Quick Start are included.
